10.14. SCCP users Table
Prev | Chapter 10. Customizing Wireshark | Next

## 10.14. SCCP users Table

Wireshark uses this table to map specific protocols to a certain DPC/SSN combination for SCCP.

This table is handled by an Section 10.7, “User Table” with the following fields.

Network Indicator

  An Integer representing the network indicator for which this association is valid.

Called DPCs

  An range of integers representing the dpcs for which this association is valid.

Called SSNs

  An range of integers representing the ssns for which this association is valid.

User protocol

  The protocol that is carried over this association

Prev | Up | Next
10.13. PRES Users Context List | Home | 10.15. SMI (MIB and PIB) Modules