10.20. User DLTs protocol table
Prev | Chapter 10. Customizing Wireshark | Next

## 10.20. User DLTs protocol table

When a pcap file uses one of the user DLTs (147 to 162) wireshark uses this table to know which protocol(s) to use for each user DLT.

This table is handled by an Section 10.7, “User Table” with the following fields.

DLT

  One of the user dlts.

Payload protocol

  This is the name of the payload protocol (the lowest layer in the packet data). (e.g. "eth" for ethernet, "ip" for IPv4)

Header size

  If there is a header protocol (before the payload protocol) this tells which size this header is. A value of 0 disables the header protocol.

Header protocol

  The name of the header protocol to be used (uses "data" as default).

Trailer size

  If there is a trailer protocol (after the payload protocol) this tells which size this trailer is. A value of 0 disables the trailer protocol.

Trailer protocol

  The name of the trailer protocol to be used (uses "data" as default).

Prev | Up | Next
10.19. Tektronix K12xx/15 RF5 protocols Table | Home | Chapter 11. Lua Support in Wireshark