6.11. Ignoring packets
Prev | Chapter 6. Working with captured packets | Next

## 6.11. Ignoring packets

You can ignore packets in the "Packet List" pane. Wireshark will then pretend that this packets does not exist in the capture file. An ignored packet will be shown with white background and gray foreground, regardless of the coloring rules set.

| Warning!
The packet ignored marks are not stored in the capture file or anywhere else, so all packet ignored marks will be lost if you close the capture file.

There are three functions to manipulate the ignored state of a packet:

- Ignore packet (toggle) toggles the ignored state of a single packet.

- Ignore all displayed packets set the ignored state of all displayed packets.

- Un-Ignore all packets reset the ignored state of all packets.

These ignore functions are available from the "Edit" menu, and the "Ignore packet (toggle)" function is also available from the pop-up menu of the "Packet List" pane.

Prev | Up | Next
6.10. Marking packets | Home | 6.12. Time display formats and time references