10.17. SNMP Enterprise Specific Trap Types
Prev | Chapter 10. Customizing Wireshark | Next

## 10.17. SNMP Enterprise Specific Trap Types

Wireshark uses this table to map specific-trap values to user defined descriptions in a Trap PDU. The description is shown in the packet details specific-trap element.

This table is handled by an Section 10.7, “User Table” with the following fields.

Enterprise OID

  The object identifier representing the object generating the trap.

Trap Id

  An Integer representing the specific-trap code.

Description

  The description to show in the packet details.

Prev | Up | Next
10.16. SMI (MIB and PIB) Paths | Home | 10.18. SNMP users Table